SA Kuka Robot Deployment

**XML Channel configuration and Data format files (C:\KRC\Roboter\INIT)**

RAC.xml

RAC+.xml

XmlApiConfig.xml (set tcp/ip address and port of remote access computer – secondary fixed ip on remote computer)

**KRL Client Communication (C:\KRC\Roboter\KRC\R1\Program)**

SAKRL.dat

SAKRL.src

**KRL Client motion programs (called by SAKRL.SRC C:\KRC\Roboter\KRC\R1\Program)**

MoveToFrame.SRC and .DAT

MoveToJointSet.SRC and .DAT

HitEStop.SRC

**VxWorks Communication Configuration (C:\Windows)**

vxWin.ini (robot controller VxWorks tcp/ip address modified under e={……})

**Server application and data format files on remote computer**

SARobotDriver.exe

SA Robot Driver.exe.manifest

KukaCoreInterface.dll

RACData.xml

**Global Data (c:\KRC\Roboter\KRC\R1\System)**

$config.dat